id: | webserver
description: | Desktop Computer
width: | 32 bits
capabilities: | smbios-2.4 dmi-2.4
configuration: |
boot | = | normal
chassis | = | desktop
uuid | = | 3A02BA42-87FB-11DD-AE6A-0013D4D9C938

id: | core
description: | Motherboard
product: | DG43NB
vendor: | Intel Corporation
physical id: | 0
version: | AAE34877-402
serial: | USNB839001TF
slot: | To be filled by O.E.M.

id: | firmware
description: | BIOS
vendor: | Intel Corp.
physical id: | 0
version: | NBG4310H.86A.0074.2009.0109.1614 (01/09/2009)
size: | 64KiB
capacity: | 960KiB
capabilities: | pci upgrade shadowing escd cdboot bootselect socketedrom edd int13floppy1200 int13floppy720 int13floppy2880 int5printscreen int9keyboard int14serial int17printer int10video acpi ls120boot zipboot biosbootspecification

id: | cpu
description: | CPU
product: | Pentium(R) Dual-Core CPU E5200 @ 2.50GHz
vendor: | Intel Corp.
physical id: | 4
bus info: | cpu@0
version: | 6.7.6
serial: | 0001-0676-0000-0000-0000-0000
slot: | LGA775
size: | 2500MHz
capacity: | 4GHz
width: | 64 bits
clock: | 200MHz
capabilities: | fpu fpu_exception wp vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush dts acpi mmx fxsr sse sse2 ss ht tm pbe nx x86-64 constant_tsc arch_perfmon pebs bts pni monitor ds_cpl est tm2 ssse3 cx16 xtpr lahf_lm
configuration: |
id | = | 1

id: | cache:0
description: | L1 cache
physical id: | 5
slot: | L1-Cache
size: | 32KiB
capacity: | 32KiB
capabilities: | internal write-back unified

id: | cache:1
description: | L2 cache
physical id: | 6
slot: | L2-Cache
size: | 2MiB
capacity: | 2MiB
capabilities: | internal varies unified

id: | logicalcpu:0
description: | Logical CPU
physical id: | 1.1
width: | 64 bits
capabilities: | logical

id: | logicalcpu:1
description: | Logical CPU
physical id: | 1.2
width: | 64 bits
capabilities: | logical

id: | memory
description: | System Memory
physical id: | 2d
slot: | System board or motherboard
size: | 4GiB

id: | bank:0
description: | DIMM Synchronous 800 MHz (1.2 ns)
product: | PartNum0
vendor: | Manufacturer0
physical id: | 0
serial: | SerNum0
slot: | CHANNEL_A
size: | 2GiB
width: | 64 bits
clock: | 800MHz (1.2ns)

id: | bank:1
description: | DIMM Synchronous 800 MHz (1.2 ns)
product: | PartNum2
vendor: | Manufacturer2
physical id: | 1
serial: | SerNum2
slot: | CHANNEL_B
size: | 2GiB
width: | 64 bits
clock: | 800MHz (1.2ns)

id: | pci
description: | Host bridge
product: | 4 Series Chipset DRAM Controller
vendor: | Intel Corporation
physical id: | 100
bus info: | pci@0000:00:00.0
version: | 03
width: | 32 bits
clock: | 33MHz
configuration: |
driver | = | agpgart-intel
module | = | intel_agp

id: | display:0
description: | VGA compatible controller
product: | 4 Series Chipset Integrated Graphics Controller
vendor: | Intel Corporation
physical id: | 2
bus info: | pci@0000:00:02.0
version: | 03
width: | 64 bits
clock: | 33MHz
capabilities: | msi pm vga_controller bus_master cap_list
configuration: |
latency | = | 0

id: | display:1
description: | Display controller
product: | 4 Series Chipset Integrated Graphics Controller
vendor: | Intel Corporation
physical id: | 2.1
bus info: | pci@0000:00:02.1
version: | 03
width: | 64 bits
clock: | 33MHz
capabilities: | pm bus_master cap_list
configuration: |
latency | = | 0

id: | communication
description: | Communication controller
product: | 4 Series Chipset HECI Controller
vendor: | Intel Corporation
physical id: | 3
bus info: | pci@0000:00:03.0
version: | 03
width: | 64 bits
clock: | 33MHz
capabilities: | pm msi bus_master cap_list
configuration: |
latency | = | 0

id: | network
description: | Ethernet interface
product: | 82567V-2 Gigabit Network Connection
vendor: | Intel Corporation
physical id: | 19
bus info: | pci@0000:00:19.0
logical name: | eth0
version: | 00
serial: | 00:1c:c0:91:e6:7c
size: | 100MB/s
capacity: | 1GB/s
width: | 32 bits
clock: | 33MHz
capabilities: | pm msi bus_master cap_list ethernet physical tp 10bt 10bt-fd 100bt 100bt-fd 1000bt-fd autonegotiation
configuration: |
autonegotiation | = | on
broadcast | = | yes
driver | = | e1000e
driverversion | = | 0.3.3.3-k2
duplex | = | full
firmware | = | 1.8-5
ip | = | 192.168.102.3
latency | = | 0
link | = | yes
module | = | e1000e
multicast | = | yes
port | = | twisted pair
speed | = | 100MB/s

id: | usb:0
description: | USB Controller
product: | 82801JI (ICH10 Family) USB UHCI Controller #4
vendor: | Intel Corporation
physical id: | 1a
bus info: | pci@0000:00:1a.0
version: | 00
width: | 32 bits
clock: | 33MHz
capabilities: | uhci bus_master cap_list
configuration: |
driver | = | uhci_hcd
latency | = | 0
module | = | uhci_hcd

id: | usbhost
product: | UHCI Host Controller
vendor: | Linux 2.6.26-2-686-bigmem uhci_hcd
physical id: | 1
bus info: | usb@1
logical name: | usb1
version: | 2.06
capabilities: | usb-1.10
configuration: |
driver | = | hub
slots | = | 2
speed | = | 12.0MB/s

id: | usb:1
description: | USB Controller
product: | 82801JI (ICH10 Family) USB UHCI Controller #5
vendor: | Intel Corporation
physical id: | 1a.1
bus info: | pci@0000:00:1a.1
version: | 00
width: | 32 bits
clock: | 33MHz
capabilities: | uhci bus_master cap_list
configuration: |
driver | = | uhci_hcd
latency | = | 0
module | = | uhci_hcd

id: | usbhost
product: | UHCI Host Controller
vendor: | Linux 2.6.26-2-686-bigmem uhci_hcd
physical id: | 1
bus info: | usb@2
logical name: | usb2
version: | 2.06
capabilities: | usb-1.10
configuration: |
driver | = | hub
slots | = | 2
speed | = | 12.0MB/s

id: | usb:2
description: | USB Controller
product: | 82801JI (ICH10 Family) USB UHCI Controller #6
vendor: | Intel Corporation
physical id: | 1a.2
bus info: | pci@0000:00:1a.2
version: | 00
width: | 32 bits
clock: | 33MHz
capabilities: | uhci bus_master cap_list
configuration: |
driver | = | uhci_hcd
latency | = | 0
module | = | uhci_hcd

id: | usbhost
product: | UHCI Host Controller
vendor: | Linux 2.6.26-2-686-bigmem uhci_hcd
physical id: | 1
bus info: | usb@3
logical name: | usb3
version: | 2.06
capabilities: | usb-1.10
configuration: |
driver | = | hub
slots | = | 2
speed | = | 12.0MB/s

id: | usb:3
description: | USB Controller
product: | 82801JI (ICH10 Family) USB2 EHCI Controller #2
vendor: | Intel Corporation
physical id: | 1a.7
bus info: | pci@0000:00:1a.7
version: | 00
width: | 32 bits
clock: | 33MHz
capabilities: | pm debug ehci bus_master cap_list
configuration: |
driver | = | ehci_hcd
latency | = | 0
module | = | ehci_hcd

id: | usbhost
product: | EHCI Host Controller
vendor: | Linux 2.6.26-2-686-bigmem ehci_hcd
physical id: | 1
bus info: | usb@6
logical name: | usb6
version: | 2.06
capabilities: | usb-2.00
configuration: |
driver | = | hub
slots | = | 6
speed | = | 480.0MB/s

id: | multimedia
description: | Audio device
product: | 82801JI (ICH10 Family) HD Audio Controller
vendor: | Intel Corporation
physical id: | 1b
bus info: | pci@0000:00:1b.0
version: | 00
width: | 64 bits
clock: | 33MHz
capabilities: | pm msi pciexpress bus_master cap_list
configuration: |
driver | = | HDA Intel
latency | = | 0
module | = | snd_hda_intel

id: | pci:0
description: | PCI bridge
product: | 82801JI (ICH10 Family) PCI Express Port 1
vendor: | Intel Corporation
physical id: | 1c
bus info: | pci@0000:00:1c.0
version: | 00
width: | 32 bits
clock: | 33MHz
capabilities: | pci pciexpress msi pm normal_decode bus_master cap_list
configuration: |
driver | = | pcieport-driver

id: | pci:1
description: | PCI bridge
product: | 82801JI (ICH10 Family) PCI Express Port 4
vendor: | Intel Corporation
physical id: | 1c.3
bus info: | pci@0000:00:1c.3
version: | 00
width: | 32 bits
clock: | 33MHz
capabilities: | pci pciexpress msi pm normal_decode bus_master cap_list
configuration: |
driver | = | pcieport-driver

id: | ide
description: | IDE interface
product: | JMB368 IDE controller
vendor: | JMicron Technologies, Inc.
physical id: | 0
bus info: | pci@0000:02:00.0
version: | 00
width: | 32 bits
clock: | 33MHz
capabilities: | ide pm pciexpress bus_master cap_list
configuration: |
driver | = | JMicron IDE
latency | = | 0
module | = | jmicron

id: | ide:0
description: | IDE Channel 0
physical id: | 0
bus info: | ide@0
logical name: | ide0
clock: | 33MHz

id: | ide:1
description: | IDE Channel 1
physical id: | 1
bus info: | ide@1
logical name: | ide1
clock: | 33MHz

id: | usb:4
description: | USB Controller
product: | 82801JI (ICH10 Family) USB UHCI Controller #1
vendor: | Intel Corporation
physical id: | 1d
bus info: | pci@0000:00:1d.0
version: | 00
width: | 32 bits
clock: | 33MHz
capabilities: | uhci bus_master cap_list
configuration: |
driver | = | uhci_hcd
latency | = | 0
module | = | uhci_hcd

id: | usbhost
product: | UHCI Host Controller
vendor: | Linux 2.6.26-2-686-bigmem uhci_hcd
physical id: | 1
bus info: | usb@4
logical name: | usb4
version: | 2.06
capabilities: | usb-1.10
configuration: |
driver | = | hub
slots | = | 2
speed | = | 12.0MB/s

id: | usb:5
description: | USB Controller
product: | 82801JI (ICH10 Family) USB UHCI Controller #2
vendor: | Intel Corporation
physical id: | 1d.1
bus info: | pci@0000:00:1d.1
version: | 00
width: | 32 bits
clock: | 33MHz
capabilities: | uhci bus_master cap_list
configuration: |
driver | = | uhci_hcd
latency | = | 0
module | = | uhci_hcd

id: | usbhost
product: | UHCI Host Controller
vendor: | Linux 2.6.26-2-686-bigmem uhci_hcd
physical id: | 1
bus info: | usb@5
logical name: | usb5
version: | 2.06
capabilities: | usb-1.10
configuration: |
driver | = | hub
slots | = | 2
speed | = | 12.0MB/s

id: | usb:6
description: | USB Controller
product: | 82801JI (ICH10 Family) USB UHCI Controller #3
vendor: | Intel Corporation
physical id: | 1d.2
bus info: | pci@0000:00:1d.2
version: | 00
width: | 32 bits
clock: | 33MHz
capabilities: | uhci bus_master cap_list
configuration: |
driver | = | uhci_hcd
latency | = | 0
module | = | uhci_hcd

id: | usbhost
product: | UHCI Host Controller
vendor: | Linux 2.6.26-2-686-bigmem uhci_hcd
physical id: | 1
bus info: | usb@7
logical name: | usb7
version: | 2.06
capabilities: | usb-1.10
configuration: |
driver | = | hub
slots | = | 2
speed | = | 12.0MB/s

id: | usb:7
description: | USB Controller
product: | 82801JI (ICH10 Family) USB2 EHCI Controller #1
vendor: | Intel Corporation
physical id: | 1d.7
bus info: | pci@0000:00:1d.7
version: | 00
width: | 32 bits
clock: | 33MHz
capabilities: | pm debug ehci bus_master cap_list
configuration: |
driver | = | ehci_hcd
latency | = | 0
module | = | ehci_hcd

id: | usbhost
product: | EHCI Host Controller
vendor: | Linux 2.6.26-2-686-bigmem ehci_hcd
physical id: | 1
bus info: | usb@8
logical name: | usb8
version: | 2.06
capabilities: | usb-2.00
configuration: |
driver | = | hub
slots | = | 6
speed | = | 480.0MB/s

id: | pci:2
description: | PCI bridge
product: | 82801 PCI Bridge
vendor: | Intel Corporation
physical id: | 1e
bus info: | pci@0000:00:1e.0
version: | 90
width: | 32 bits
clock: | 33MHz
capabilities: | pci subtractive_decode bus_master cap_list

id: | network:0
description: | Ethernet interface
product: | RTL-8169 Gigabit Ethernet
vendor: | Realtek Semiconductor Co., Ltd.
physical id: | 0
bus info: | pci@0000:03:00.0
logical name: | eth1
version: | 10
serial: | 00:40:f4:e9:82:e2
size: | 100MB/s
capacity: | 1GB/s
width: | 32 bits
clock: | 66MHz
capabilities: | pm bus_master cap_list ethernet physical tp 10bt 10bt-fd 100bt 100bt-fd 1000bt-fd autonegotiation
configuration: |
autonegotiation | = | on
broadcast | = | yes
driver | = | r8169
driverversion | = | 2.2LK-NAPI
duplex | = | full
ip | = | 91.147.208.50
latency | = | 64
link | = | yes
maxlatency | = | 64
mingnt | = | 32
module | = | r8169
multicast | = | yes
port | = | twisted pair
speed | = | 100MB/s

id: | network:1
description: | Ethernet interface
product: | RTL-8139/8139C/8139C+
vendor: | Realtek Semiconductor Co., Ltd.
physical id: | 2
bus info: | pci@0000:03:02.0
logical name: | eth2
version: | 10
serial: | 00:14:78:04:7e:7f
size: | 100MB/s
capacity: | 100MB/s
width: | 32 bits
clock: | 33MHz
capabilities: | pm bus_master cap_list ethernet physical tp mii 10bt 10bt-fd 100bt 100bt-fd autonegotiation
configuration: |
autonegotiation | = | on
broadcast | = | yes
driver | = | 8139too
driverversion | = | 0.9.28
duplex | = | full
latency | = | 32
link | = | yes
maxlatency | = | 64
mingnt | = | 32
module | = | 8139too
multicast | = | yes
port | = | MII
speed | = | 100MB/s

id: | network:2
description: | Ethernet interface
product: | RTL-8169 Gigabit Ethernet
vendor: | Realtek Semiconductor Co., Ltd.
physical id: | 4
bus info: | pci@0000:03:04.0
logical name: | eth3
version: | 10
serial: | 00:40:f4:cb:e4:68
size: | 100MB/s
capacity: | 1GB/s
width: | 32 bits
clock: | 66MHz
capabilities: | pm bus_master cap_list ethernet physical tp 10bt 10bt-fd 100bt 100bt-fd 1000bt-fd autonegotiation
configuration: |
autonegotiation | = | on
broadcast | = | yes
driver | = | r8169
driverversion | = | 2.2LK-NAPI
duplex | = | half
latency | = | 64
link | = | yes
maxlatency | = | 64
mingnt | = | 32
module | = | r8169
multicast | = | yes
port | = | twisted pair
speed | = | 100MB/s

id: | firewire
description: | FireWire (IEEE 1394)
product: | FW323
vendor: | Agere Systems
physical id: | 6
bus info: | pci@0000:03:06.0
version: | 70
width: | 32 bits
clock: | 33MHz
capabilities: | pm ohci bus_master cap_list
configuration: |
driver | = | ohci1394
latency | = | 32
maxlatency | = | 24
mingnt | = | 12
module | = | ohci1394

id: | isa
description: | ISA bridge
product: | 82801JIB (ICH10) LPC Interface Controller
vendor: | Intel Corporation
physical id: | 1f
bus info: | pci@0000:00:1f.0
version: | 00
width: | 32 bits
clock: | 33MHz
capabilities: | isa bus_master cap_list
configuration: |
latency | = | 0

id: | storage
description: | SATA controller
product: | 82801JI (ICH10 Family) SATA AHCI Controller
vendor: | Intel Corporation
physical id: | 1f.2
bus info: | pci@0000:00:1f.2
logical name: | scsi0
logical name: | scsi1
logical name: | scsi4
version: | 00
width: | 32 bits
clock: | 66MHz
capabilities: | storage msi pm ahci_1.0 bus_master cap_list emulated
configuration: |
driver | = | ahci
latency | = | 0
module | = | ahci

id: | disk:0
description: | ATA Disk
product: | ST3500418AS
vendor: | Seagate
physical id: | 0
bus info: | scsi@0:0.0.0
logical name: | /dev/sda
version: | CC34
serial: | 9VM18MXM
size: | 465GiB (500GB)
capabilities: | partitioned partitioned:dos
configuration: |
ansiversion | = | 5
signature | = | 0006df25

id: | volume
description: | EXT3 volume
vendor: | Linux
physical id: | 1
bus info: | scsi@0:0.0.0,1
logical name: | /dev/sda1
version: | 1.0
serial: | 84e35524-2085-44f9-ae09-57f9784bd27a
size: | 465GiB
capacity: | 465GiB
capabilities: | primary bootable multi journaled extended_attributes large_files huge_files recover ext3 ext2 initialized
configuration: |
created | = | 2009-02-10 20:10:20
filesystem | = | ext3
modified | = | 2011-03-12 10:53:50
mounted | = | 2011-03-12 10:53:50
state | = | clean

id: | disk:1
description: | ATA Disk
product: | ST3500820AS
vendor: | Seagate
physical id: | 1
bus info: | scsi@1:0.0.0
logical name: | /dev/sdb
version: | LC11
serial: | 5QM3T4VF
size: | 465GiB (500GB)
capabilities: | partitioned partitioned:dos
configuration: |
ansiversion | = | 5
signature | = | 0006df25

id: | volume
description: | EXT3 volume
vendor: | Linux
physical id: | 1
bus info: | scsi@1:0.0.0,1
logical name: | /dev/sdb1
version: | 1.0
serial: | 84e35524-2085-44f9-ae09-57f9784bd27a
size: | 465GiB
capacity: | 465GiB
capabilities: | primary bootable multi journaled extended_attributes large_files huge_files recover ext3 ext2 initialized
configuration: |
created | = | 2009-02-10 20:10:20
filesystem | = | ext3
modified | = | 2011-03-12 10:53:50
mounted | = | 2011-03-12 10:53:50
state | = | clean

id: | cdrom
description: | DVD-RAM writer
product: | CDDVDW SH-S223F
vendor: | TSSTcorp
physical id: | 0.0.0
bus info: | scsi@4:0.0.0
logical name: | /dev/cdrom
logical name: | /dev/cdrw
logical name: | /dev/dvd
logical name: | /dev/dvdrw
logical name: | /dev/scd0
logical name: | /dev/sr0
version: | SB00
capabilities: | removable audio cd-r cd-rw dvd dvd-r dvd-ram
configuration: |
ansiversion | = | 5
status | = | nodisc

id: | serial
description: | SMBus
product: | 82801JI (ICH10 Family) SMBus Controller
vendor: | Intel Corporation
physical id: | 1f.3
bus info: | pci@0000:00:1f.3
version: | 00
width: | 64 bits
clock: | 33MHz
configuration: |
driver | = | i801_smbus
latency | = | 0
module | = | i2c_i801

id: | network:0
description: | Ethernet interface
physical id: | 1
logical name: | eth2.4
serial: | 00:14:78:04:7e:7f
capabilities: | ethernet physical
configuration: |
broadcast | = | yes
ip | = | 192.168.104.1
multicast | = | yes

id: | network:1
description: | Ethernet interface
physical id: | 2
logical name: | eth2.5
serial: | 00:14:78:04:7e:7f
capabilities: | ethernet physical
configuration: |
broadcast | = | yes
ip | = | 192.168.105.1
multicast | = | yes

id: | network:2
description: | Ethernet interface
physical id: | 3
logical name: | eth2.6
serial: | 00:14:78:04:7e:7f
capabilities: | ethernet physical
configuration: |
broadcast | = | yes
ip | = | 192.168.106.1
multicast | = | yes

id: | network:3
description: | Ethernet interface
physical id: | 4
logical name: | eth2.7
serial: | 00:14:78:04:7e:7f
capabilities: | ethernet physical
configuration: |
broadcast | = | yes
ip | = | 192.168.107.1
multicast | = | yes